<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.28.2-Firenze">
  <identifier></identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title></title>
  <abstract></abstract>
  <contact>
    <name></name>
    <organization></organization>
    <position></position>
    <voice></voice>
    <fax></fax>
    <email></email>
    <role></role>
  </contact>
  <links/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>PROJCRS["Pulkovo 1942(58) / Stereo70",BASEGEOGCRS["Pulkovo 1942(58)",DATUM["Pulkovo 1942(58)",ELLIPSOID["Krassowsky 1940",6378245,298.3,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4179]],CONVERSION["Stereo 70",METHOD["Oblique Stereographic",ID["EPSG",9809]],PARAMETER["Latitude of natural origin",46,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8801]],PARAMETER["Longitude of natural origin",25,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8802]],PARAMETER["Scale factor at natural origin",0.99975,SCALEUNIT["unity",1],ID["EPSG",8805]],PARAMETER["False easting",500000,LENGTHUNIT["metre",1],ID["EPSG",8806]],PARAMETER["False northing",500000,LENGTHUNIT["metre",1],ID["EPSG",8807]]],CS[Cartesian,2],AXIS["northing (X)",north,ORDER[1],LENGTHUNIT["metre",1]],AXIS["easting (Y)",east,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Engineering survey, topographic mapping."],AREA["Romania - onshore and offshore."],BBOX[43.44,20.26,48.27,31.41]],ID["EPSG",3844]]</wkt>
      <proj4>+proj=sterea +lat_0=46 +lon_0=25 +k=0.99975 +x_0=500000 +y_0=500000 +ellps=krass +units=m +no_defs</proj4>
      <srsid>27265</srsid>
      <srid>3844</srid>
      <authid>EPSG:3844</authid>
      <description>Pulkovo 1942(58) / Stereo70</description>
      <projectionacronym>sterea</projectionacronym>
      <ellipsoidacronym>EPSG:7024</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial miny="0" maxx="0" dimensions="2" maxz="0" minx="0" maxy="0" crs="EPSG:3844" minz="0"/>
    <temporal>
      <period>
        <start></start>
        <end></end>
      </period>
    </temporal>
  </extent>
</qgis>
